|  |  |
| --- | --- |
|

|  |
| --- |
| **RECORD OF VISUAL HATCH COVER SURVEY** |

 |
|   |
|
|
|
|
|
|
|  |
|  |
|  |
|  |
| All correspondence should be addressed to the Managers |
|   |  |  |  |  |  |  |  |   |
|   |  |  Name of ship |   |   |   |  |   |
|   |  |  Operator |   |   |   |   |  |   |
|   |  |  Type of ship |   |   |   |  |   |
|   |  |  Year and country of build |   |   |  |   |
|   |  |  Flag |   |   |   |   |  |   |
|   |  |  Gross tonnage |   |   |   |  |   |
|   |  |  Classification Society |   |   |   |  |   |
|   |  |  |  |  |  |  |  |   |
|   |  |  |  |  |  |  |  |   |
|   |  Date(s) and place(s) of survey |  Date |  Place |   |
|   |   |  |   |   |   |   |   |   |
|   |   |   |   |   |   |   |   |   |
|   |  Name of Survey Company |   |   |   |   |   |
|   |  Name of Surveyor |   |   |   |   |   |   |
|   |   |   |   |   |   |   |   |   |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **ABC** |   |   | **NOT** | **NOT** | **YES** | **NO** |
| **No.** |   |   | **CHECKED** | **RELEVANT** |   |   |
| S1 |  Can ship's staff confirm if the holds have been sea water washed? |  |  |   |   |
| S2 |  Can ship's staff confirm if the holds have been fresh water rinsed? |  |  |   |   |
| S3 |  Was the ship's certification relating to hatch cover weathertightness (Class survey) valid?  |  |  |   |   |
|   |  [e.g. LR require this annually under  |  |  |   |   |
|   |  Rule: Part 1, Chapter 3, Section 2.2.2(a)] |  |  |   |   |
| 46 |  Are external vents, sounding pipes and their closing appliances in good condition and correctly labelled? |  |  |   |   |
|   |  |  |  |   |   |
| 47 |  Are all external watertight closures of deck openings in satisfactory condition and well maintained?  |  |  |   |   |
|   |  (e.g. Access hatches) |  |  |   |   |
| 59 | Are these items in  |  hatch cover panels / pontoons |   |   |   |   |
| 60 | satisfactory condition? |  hinge pins, locators, wheels & axles |   |   |   |   |
| 61 |   |  hatch cover seal packing or tarpaulins |   |   |   |   |
| 62 |   |  seal packing channels |   |   |   |   |
| 63 |  |  all cleats, wedges and securing bars |   |   |   |   |
| 64 |  |  compression bars |   |   |   |   |
| 65 |  |  coamings |   |   |   |   |
| 66 |  |  drains and non-return arrangements |   |   |   |   |
| 67 |   |  coaming tops and trackways |   |   |   |   |
| 68 |  Are hatch covers free from the use of additional sealing methods?  |   |   |   |   |
|   |  (e.g. sealing tape, expanding foam, cement and non-class approved systems)  |   |   |   |   |
| 69 |  Are hatch coaming internal surfaces free of recent leakage  |   |   |   |   |
|   |  indications? |   |   |   |   |   |
| 70 |  Do hatch cover operating systems appear in satisfactory |   |   |   |   |
|   |  condition? |   |   |   |   |   |
| 140 |  Can ship's staff confirm that records of regular testing of bilge systems are kept; including alarms? |   |   |   |   |
|   |  |   |   |   |   |
| 141 |  Can ship's staff confirm that bilge soundings are logged daily? |   |   |   |   |